Date		Version	Note
===============+========+=============================================================================================
2005.08.18	1.163	1. Fix shared-key authentication bug.

2005.08.24	1.164	1. Fix AP mode shared-key authentication bug.

2005.08.24	1.165	1. Fix the bug about setting invalid channel number via OID.

2005.08.25	1.17	1. Regular revision.

2005.10.07	1.180	1. Implement AES and WPA2.

2005.10.13	1.181	1. Fix the bug about too man buffers in a NDIS_PACKET to send.
			2. Fix the bug of RFOff failed at initializaion.

2005.10.17	1.182	1. Fix the bug about key length of AES on Win98SE/WinME.

2005.10.19	1.183	1. Fix OS hangs when we plug two 8187 on one machine.

2005.10.24	1.184	1. Fix the bug about WOL.

2005.10.27	1.185	1. Fix the bug about WOL from S5.

2005.11.02	1.186	1. Add turbo mode feature.

2005.11.04	1.187	1. Solve WPA-none AES issue in win98se with eappkt9x.vxd.

2005.11.17	1.188	1. Fix the bug about bluescreen when we unplug during chariot throughput testing.
			2. Fix the bug about too long time to unload driver when we unplug just after plugged.
			3. Change turbo mode default setting to "Enable."
			4. Add feature: use pin "GPIO1" to turn on/off RF for buletooth.

2005.11.18	1.189	1. Fix a bug that we can not scan to any AP.

2005.11.21	1.190	1. Modify length of passphrase in AP mode: 8-63.

2005.11.29	1.191	1. Implement EzConfig/AutoConfig with RTL8186.
			2. Use hardware beacon in AP mode.

2005.12.09	1.192	1. Fix a bug about privacy bit and capability setting in AP mode WEP encryption.
			2. Revise the EIFS setting.
			3. Fix a bug about OS hanged when 8187 unplugged on Windows ME.

2005.12.09	1.193	1. Implement OID for qurying HW RFOff status.
			2. Regular revision for WHQL test.

2005.12.12	1.194	1. Fix a bug in GPIO pin RF changing.
			2. Revise the default EIFS/DIFS setting.

2005.12.14	1.195	1. Disable turbo mode in Ad-Hoc mode.

2005.12.16	1.196	1. Revise the response rate.

2005.12.19	1.197	1. Revise EIFS setting.
			2. Modify parameters with Zebra2.

2005.12.27	1.198	1. Auto select channel of SW AP.

2005.12.28	1.199	1. Revise auto select channel mechanism.

2006.01.20	1.200	1. Fix Cisco 1242 compatability issue.

2006.01.24	1.201	1. Add ASUS 8187 VID/PID.
			2. Handle the registy entries: 	MaxPktSize, ShortRetryLimit,
			LongRetryLimit, LongRetryLimit, RTSThresh.

2006.01.24	1.202	1. Replace the parameter description "WiFi 11b IBSS" with "IBSS Default 11b Mode".

2006.01.26	1.203	1. Revise AP mode beacon for ASUS WiFi phone power save mode.
			2. Revise auto select channel setting.

2006.02.14	1.204	1. Solve USB 1.1 Rx performance issue.

2006.02.16	1.205	1. Solve USB 1.1 Rx performance issue.

2006.02.16	1.206	1. Hidde SSID.
			2. Locked STA MAC address.

2006.02.16	1.207	1. Revise Z2 parameter.
			2. Handle class2 and class3 error on AP mode.

2006.02.27	1.208	1. Change default value of STA LiveTime in AP mode.

2006.03.01	1.209	1. Fix the error in rtl8187.rc on v1208.

2006.03.03	1.210	1. Review 802.11 power management.
			2. Review SW AP mode.
			3. Improve throughput when B mode STA in current IBSS.

2006.03.07	1.211	1. Revise AP mode beacon behavior.

2006.03.09	1.212	1. Fix the bug when we disable device on Windows 2000.
			2. Revise Z2 parameter.

2006.03.16	1.213	1. Allow device to use g mode under USB 1.1.

2006.03.10	1.214	1. Return device description from that of INF.
			2. Smooth Z2 signal strength report.
			3. Smooth data rate report.

2006.03.10	1.215	1. Fix a bug about TBTT calculation.

2006.03.21	1.216	1. Solve the problem OS hangs on Win98Se/ME since v1203.
			2. Revise LED behavior (SW LED mode 1).
			3. Handle the EEPROMID=0xAABB

2006.03.22	1.217	1. Fix a bug in auto turbo mode with 8186.

2006.03.22	1.218	1. Allow device to use g mode under USB 1.1.
			2. Revise SW AP beacon behavior.

2006.04.04	1.219	1. Turbo mode spec cahnge.
			2. Fix Tx stuck bug encountered in WHQL test.
			3. Implment signal quality report.

2006.04.12	1.221	1. Implement SW_LED_MODE2 for AzWave 8187 minicard.
			2. Fix the bug that OID_RT_FORCED_DATA_RATE can't set to Auto(0).
			3. Fix a fragmentation sequnece number bug.
			4. Correct scanned IBSS encryption and authentication status shown on UI.

2006.04.18	1.222	1. Implement Antenna Diversity for minicard interface.
			2. Implement per-sta fixed data rate in SW AP mode.

2006.04.21	1.223	1. Fix IBSS throughput issue.
			2. Customized for Sercomm.

2006.04.26	1.224	1. Turn off auto-rate fallback mechanism when destination STA is configured to 
			be fixed data rate.

2006.05.02	1.225	1. Don't display surprisely remove icon for minicard.

2006.05.05	1.226	1. Review counter measure flow for WPA2 logo.
			2. Fix HW RF bug at AP mode.
			3. Add AP mode rate adaptive.
			4. Perform WOL on every RF.

2006.05.09	1.227	1. Fix S3 resume issue.

2006.05.10	1.228	1. Revise adding WEP key.
			2. Fix the bug about TxOK when RF is off.

2006.05.12	1.229	1. Revise for WPA2.
			2. Fix 8187 minicard RF Off issue.
			3. Fix the bug about AP mode auto select channel mechanism.
			4. Implment OID for new no registry UI architecture.

2006.05.30	1.230	1. Fix AZ minicard LED bug when switch to HW RF off.
			2. Improve AP mode rate-Adaptive.
			3. Revise for WiFi WPA2 Mandatory Testplan v1.2.
			4. Add an CustomID, 0x03, for HW LED.	
			5. Fix Win98SE/ME IBSS cause OS hangs.
			6. Revise for HCT test.

2006.06.10	1.231	1. Fix Rx throughput issue.

2006.06.22	1.232	1. Support WDS.

2006.06.23	1.233	1. Fix XP SP1 flash disk unplug issue.
			2. Fix the bug scanning few AP after ping over 12 hr.

2006.06.30	1.234	1. Fix X64 WHQL bug found in v1233.

2006.07.04	1.235	1. Speed up initialization on USB 1.1.
			2. Revise rate adaptive mechanism.
			3. Customize IBSS wireless mode for wg111v2 on USB 1.1.

2006.07.18	1.236	1. Add Surecom VID/PID.

2006.07.20	1.237	1. Add Sercomm VID/PID.
